Atari Lunar Lander

Many if not all Lunar Lander games produced for sale in the USA do not have
the ROM with the part number 034597-01.  This ROM is used for non-English
messages only.  This ROM is not currently available in the archive.  For use
with the simulator, there is a file 034597.01.fake, which contains 2K bytes of
hexadecimal FF.

There are two known versions of the code ROMs (b1, cd1, de1, and f1), which
have part numbers ending in -01 and -02.  The same vector ROMs are used with
both sets of code.

All EPROMs are type 2716 (but not TMS 2716).  Some boards may use bipolar
PROMs instead of EPROMs.  It is easiest to simply replace the PROMs with
EPROMs if the EPROM sockets are loaded.  See the operator's manual for details.

loc  part num   cksm  filename   
---  ---------  ----  ---------
b1   034569-01  69fa  034569.01  
cd1  034570-01  7dde  034570.01  
de1  034571-01  d650  034571.01  
f1   034572-01  1ff8  034572.01  
                                 
     034597-01
np3  034598-01  0342  034598.01  
r3   034599-01  f04a  034599.01  

b1   034569-02  6784  034569.02
cd1  034570-02  7dde  034570.02  (note: same contents as 034570-01)
de1  034571-02  d40e  034571.02
f1   034572-02  2482  034572.02
